**Frankfurt – Prolight&Sound 2014**

**Dotz Matrix** – Representing the next evolution in LED technology, this Wash/Blinder matrix panel is powered by 16 x 30-watt 3-in-1 color-mixing RGB COB LEDs (configured in 4 rows x 4 LEDs). The difference in COB technology vs. SMDs is that multiple COB LED diodes are directly mounted on the circuit board as one lighting module, so interconnection lengths are shortened, resulting in greater output from a smaller illumination source, more even light distribution, better color homogenization and improved heat dissipation. In addition to its super-charged output, the Dotz Matrix offers pixel mapping capabilities with 4 pixel flipping options for stunning visual effects. Great for stage lighting, bands and nightclubs, it also has a full complement of other pro features, including: a massive 60° beam angle, 5 selectable dimming curves, strobe/pulse effect, built-in shows and color macros, DMX control (5 DMX channel mode options), RDM (Remote Device Management), and 4 operational modes.

**For more information Contact ADJ Europe:    
Phone: +31 45 546 85 00  
Fax: +31 45 546 85 99  
address: Junostraat 2, 6468EW Kerkrade, The Netherlands**[**www.adj.com**](http://www.adj.com)

**Facebook/adjeurope**