**Frankfurt – Prolight&Sound 2014**

**FX Beam** – Another example from ADJ that “good things come in small packages,” the FX Beam is a micro pin beam effect (4.75” x 4.75” x 6”/ 119 x 119 x 148 mm) with a narrow 3°angle that’s great for spotting displays and dinner tables, as well as for use in multiples to create pure lighting excitement at parties and events. It features an FX mode switch on the rear panel that allows users to run it in Sound Active or Strobe mode, as well as a potentiometer for controlling strobe speed. A versatile fixture, the FX Beam can also be used with ADJ’s T4 or T20F chase controllers for an automated light show.

**For more information Contact ADJ Europe:    
Phone: +31 45 546 85 00  
Fax: +31 45 546 85 99  
address: Junostraat 2, 6468EW Kerkrade, The Netherlands**[**www.adj.com**](http://www.adj.com)

**Facebook/adjeurope**